**STEINEL Professional Motion detector**

**sensIQ S**

**white V3**

Dimensions (L x W x H): 128 x 114 x 74 mm; Manufacturer's Warranty: 5 years; Settings via: ETS software, Remote control, Bus, Smart Remote; With remote control: Yes; Version: white; PU1, EAN: 4007841059613; Type: Motion detectors; Application, place: Indoors, Outdoors; Application, room: multi-storey / underground car park, outdoors, warehouse, front door, all round the building, courtyard & driveway, Indoors; Colour: white; Colour, RAL: 9010; Includes corner wall mount: Yes; Installation site: wall, corner; Installation: Surface wiring, Wall, corner; Ambient temperature: -20 – 50 °C; Material: Plastic; With bus coupling: Yes; Mounting height: 2 – 5,00 m; Mounting height max.: 5,00 m; Optimum mounting height: 2 m; Detection angle: 300 °; Angle of aperture: 180 °; Sneak-by guard: Yes; Capability of masking out individual segments: Yes; Electronic scalability: No; Mechanical scalability: Yes; Reach, radial: r = 4 m (42 m²); Reach, tangential: r = 20 m (1047 m²); Twilight setting: 2 – 1000 lx; Time setting: 60 sec – 15 min; Basic light level function: Yes; Main light adjustable: 0 - 100 %; Twilight setting TEACH: Yes; Constant-lighting control: Yes; KNX functions: Light output 2x, Presence output, Light level, Constant-lighting control, Basic light level function, Photo-cell controller, Close range, Individual pyro evaluation, Logic gate; Interconnection: Yes; Type of interconnection: Master/master, Master/slave; Interconnection via: KNX bus; Rated current: 10 mA

**Manufacturer** Steinel

**Prod. No.** 059613

**Ordering designation** sensIQ S white

Deliver, install and set ready for operation