**STEINEL Professional Presence detector**

**HF 360-2**

**DALI-2 APC - surface**

Dimensions (L x W x H): 57 x 123 x 123 mm; With motion detector: Yes; Manufacturer's Warranty: 5 years; Settings via: Bluetooth; With remote control: No; Version: DALI-2 APC - surface; PU1, EAN: 4007841064273; Type: Presence detector; Application, place: Indoors; Application, room: function room / ancillary room, kitchenette, stairwell, WC / washroom, Indoors; Colour: white; Colour, RAL: 9003; Includes corner wall mount: No; Installation site: ceiling; Installation: Surface wiring, Ceiling; IP-rating: IP54; Ambient temperature: -25 – 50 °C; Material: Plastic; Mains power supply: 220 – 240 V / 50 – 60 Hz; Power supply, detail: max. 64 users; Number of Dali users: 64; Steuerausgang, Dali: Addressable / broadcast 64 electronic ballasts; Technology, sensors: High frequency, Photo-cell controller; Mounting height: 2,50 – 4,00 m; Mounting height max.: 4,00 m; Optimum mounting height: 2,8 m; HF-system: 5,8 GHz; Detection: also through glass, wood and stud walls; Detection angle: 360 °; Angle of aperture: 140 °; Sneak-by guard: Yes; Capability of masking out individual segments: No; Electronic scalability: Yes; Mechanical scalability: No; Reach, radial: Ø 12 m (113 m²); Reach, tangential: Ø 12 m (113 m²); Transmitter power: < 1 mW; Functions: Semi-/fully automatic, Constant-lighting control, Lighting scenario, Master/slave override, Neighbouring group function, TouchDIM function, Selecting programmed lighting scenarios, Constant-lighting control ON-OFF, Manual ON / ON-OFF, Normal / test mode; Twilight setting: 2 – 2000 lx; Time setting: 10 sec – 60 min; Basic light level function: Yes; Basic light level function time: 1-60 min, all night; Main light adjustable: 50 - 100 %; Twilight setting TEACH: Yes; Constant-lighting control: Yes; Interconnection: Yes; Type of interconnection: Master/slave; Interconnection via: Bluetooth, DALI bus

**Manufacturer** Steinel

**Prod. No.** 064273

**Ordering designation** HF 360-2 DALI-2 APC - surface

Deliver, install and set ready for operation