**STEINEL Professional Presence detector**

**HF 360-2**

**BT IPD - surface**

Dimensions (L x W x H): 57 x 123 x 123 mm; With motion detector: Yes; Manufacturer's Warranty: 5 years; Settings via: Bluetooth; With remote control: No; Version: BT IPD - surface; PU1, EAN: 4007841064426; Type: Presence detector; Application, place: Indoors; Application, room: function room / ancillary room, kitchenette, stairwell, WC / washroom, Indoors; Colour: white; Colour, RAL: 9003; Includes corner wall mount: No; Installation site: ceiling; Installation: Surface wiring, Ceiling; IP-rating: IP54; Ambient temperature: -25 – 50 °C; Material: Plastic; Mains power supply: 220 – 240 V / 50 – 60 Hz; Power consumption: 0,5 W; Technology, sensors: High frequency, Light sensor; Mounting height: 2,50 – 4,00 m; Mounting height max.: 4,00 m; Optimum mounting height: 2,8 m; HF-system: 5,8 GHz; Detection: also through glass, wood and stud walls; Detection angle: 360 °; Angle of aperture: 140 °; Sneak-by guard: Yes; Capability of masking out individual segments: No; Electronic scalability: Yes; Mechanical scalability: No; Reach, radial: Ø 12 m (113 m²); Reach, tangential: Ø 12 m (113 m²); Transmitter power: < 1 mW; Basic light level function: No; Main light adjustable: No; Twilight setting TEACH: No; Constant-lighting control: No; Interconnection: Yes; Type of interconnection: Master/slave; Interconnection via: Bluetooth

**Manufacturer** Steinel

**Prod. No.** 064426

**Ordering designation** HF 360-2 BT IPD - surface

Deliver, install and set ready for operation