**STEINEL Professional Presence detector**

**HF 360-2**

**IP - surface**

Dimensions (L x W x H): 57 x 123 x 123 mm; With motion detector: Yes; Manufacturer's Warranty: 5 years; Settings via: Bluetooth, Web-Interface; With remote control: No; Version: IP - surface; PU1, EAN: 4007841065966; Type: Presence detector; Application, place: Indoors; Application, room: function room / ancillary room, kitchenette, stairwell, WC / washroom, Indoors; Colour: white; Colour, RAL: 9003; Includes corner wall mount: No; Installation site: ceiling; Installation: Surface wiring, Ceiling; IP-rating: IP20; Ambient temperature: -25 – 50 °C; Material: Plastic; Mains power supply: 18 – 55 V; Power supply, detail: Passive PoE SELV, standard PoE (IEEE 802.3 af); Technology, sensors: High frequency, Light sensor, Temperature, Air humidity; Mounting height: 2,50 – 4,00 m; Mounting height max.: 4,00 m; Optimum mounting height: 2,8 m; HF-system: 5,8 GHz; Detection: also through glass, wood and stud walls; Detection angle: 360 °; Angle of aperture: 140 °; Sneak-by guard: Yes; Capability of masking out individual segments: No; Electronic scalability: Yes; Mechanical scalability: No; Reach, radial: Ø 12 m (113 m²); Reach, tangential: Ø 12 m (113 m²); Transmitter power: < 1 mW; Twilight setting: 2 – 2000 lx; Basic light level function: No; Main light adjustable: No; Twilight setting TEACH: No; Constant-lighting control: No; Interconnection: Yes; Interconnection via: Bluetooth, LAN

**Manufacturer** Steinel

**Prod. No.** 065966

**Ordering designation** HF 360-2 IP - surface

Deliver, install and set ready for operation