**STEINEL Professional Presence detector**

**Dual US**

**COM1 - in-ceiling installation**

Dimensions (L x W x H): 109 x 120 x 120 mm; Manufacturer's Warranty: 5 years; Settings via: Remote control, DIP switches, Potentiometers, Smart Remote; With remote control: Yes; Version: COM1 - in-ceiling installation; PU1, EAN: 4007841079598; Type: Presence detector; Application, place: Indoors; Application, room: corridor / aisle, Indoors; Colour: white; Colour, RAL: 9010; Includes corner wall mount: No; Installation site: ceiling; Installation: In-ceiling installation, Ceiling; IP-rating: IP20; Ambient temperature: -25 – 55 °C; Material: Plastic; Mains power supply: 220 – 240 V / 50 – 60 Hz; Technology, sensors: Ultrasonic, Light sensor; Mounting height: 2,50 – 3,50 m; Mounting height max.: 3,50 m; Optimum mounting height: 2,8 m; Ultrasonic technology: 40 kHz; Detection angle: Aisle, 360 °; Angle of aperture: 180 °; Sneak-by guard: Yes; Capability of masking out individual segments: No; Electronic scalability: Yes; Mechanical scalability: No; Reach, radial: 20 x 3 m (60 m²); Reach, tangential: 20 x 3 m (60 m²); Functions: Normal / test mode, Semi-/fully automatic, Pushbutton / switch mode, Manual ON / ON-OFF; Twilight setting: 10 – 1000 lx; Time setting: 30 sec – 30 min; Basic light level function: No; Main light adjustable: No; Twilight setting TEACH: Yes; Constant-lighting control: No; Interconnection: Yes; Type of interconnection: Master/master, Master/slave; Interconnection via: Cable; Interconnection, number: max. 10 sensors

**Manufacturer** Steinel

**Prod. No.** 079598

**Ordering designation** Dual US COM1 - in-ceiling installation

Deliver, install and set ready for operation