**STEINEL Professional Sensor-switched indoor light**

**RS 10 S**

Dimensions (Ø x H): 280 x 110 mm; With lamp: No; With motion detector: Yes; Manufacturer's Warranty: 5 years; Settings via: Potentiometers; With remote control: No; PU1, EAN: 4007841730512; Application, place: Indoors; Application, room: corridor / aisle, function room / ancillary room, stairwell, WC / washroom, outdoors, Indoors; Colour: white; Installation site: wall, ceiling; Installation: Wall, Ceiling, Surface wiring; Impact resistance: IK03; IP-rating: IP44; Protection class: II; Ambient temperature: -20 – 40 °C; Housing material: Aluminium; Cover material: Glass opal; Mains power supply: 230 – 240 V / 50 Hz; Switching output 1, resistive: 800 W; Power consumption: 1,1 W; Mounting height max.: 4,00 m; HF-system: 5,8 GHz; Detection: also through glass, wood and stud walls; Capability of masking out individual segments: No; Electronic scalability: Yes; Mechanical scalability: No; Reach, radial: Ø 8 m (50 m²); Reach, tangential: Ø 8 m (50 m²); Photo-cell controller: Yes; Transmitter power: < 1 mW; Lamp: All-purpose lamp; Base: E27; Soft light start: No; Continuous light: selectable; Twilight setting: 2 – 2000 lx; Time setting: 5 sec – 15 min; Basic light level function: No; Twilight setting TEACH: No; Interconnection: Yes; Type of interconnection: Master/master; Interconnection via: Cable; Output: 60 W; Angle of aperture: 160 °; IP-rating, ceiling: IP44; Detection angle: 360 °

**Manufacturer** Steinel

**Prod. No.** 730512

**Ordering designation** RS 10 S

Deliver, install and set ready for operation