**STEINEL Professional Sensor-switched LED outdoor light**

**L 825 SC**

**Anthracite**

Dimensions (L x W x H): 157 x 331 x 95 mm; With lamp: Yes, STEINEL LED system; Manufacturer's Warranty: 5 years; With remote control: No; Version: Anthracite; PU1, EAN: 4007841059903; Application, place: Outdoors; Application, room: outdoors, front door, all round the building, terrace / balcony, courtyard & driveway; Colour: Anthracite; includes sheet of self-adhesive numbers: No; Installation site: wall; Impact resistance: IK03; IP-rating: IP44; Protection class: II; Ambient temperature: -20 – 40 °C; Housing material: Aluminium; Cover material: Plastic, opal; Mains power supply: 220 – 240 V / 50 – 60 Hz; Output: 9,7 W; Mounting height max.: 2,50 m; Slave modeselectable: No; Sneak-by guard: No; Capability of masking out individual segments: No; Electronic scalability: Yes; Mechanical scalability: No; Reach, detail: Detection zone adjustable on 2 axes; Reach, radial: r = 5 m (35 m²); Reach, tangential: r = 5 m (35 m²); Photo-cell controller: Yes; Transmitter range: 30 m; Transmitter power: < 1 mW; Luminous flux total product: 707 lm; Measured luminos flux (360°): 707 lm; Total product efficiency: 73 lm/W; Colour temperature: 3000 K; Lamp: LED cannot be replaced; Service life LED L70B50 (25°): > 60000 h; Base: without; LED cooling system: Active and Passive Thermo Control; Soft light start: Yes; Continuous light: selectable, 4h; Functions: Group parameterisation, Manual ON / ON-OFF; Twilight setting: 2 – 2000 lx; Basic light level function: Yes; Basic light level function time: 10-30 min, all night; Main light adjustable: 50 - 100 %; Interconnection: Yes; Type of interconnection: Master/master; Basic light level function in per cent: 10 – 50 %; Basic light level function percentage, from: 10 %; Basic light level function percentage, up to: 50 %; Interconnection via: Bluetooth Mesh Connect; Colour Rendering Index CRI: = 82; Optimum mounting height: 2 m; Detection angle: 160 °

**Manufacturer** Steinel

**Prod. No.** 059903

**Ordering designation** L 825 SC Anthracite

Deliver, install and set ready for operation