**STEINEL Professional Presence detector**

**IR Micro Office 6m**

**DALI-2 APC - in-ceiling installation**

Dimensions (Ø x H): 85 x 69 mm; With motion detector: Yes; Manufacturer's Warranty: 5 years; Settings via: Bluetooth; With remote control: No; Version: DALI-2 APC - in-ceiling installation; PU1, EAN: 4007841067144; Type: Presence detector; Application, place: Indoors; Application, room: Indoors, one-person office, function room / ancillary room, conference room / meeting room, duty room, recreation room, kitchenette; Colour: white; Colour, RAL: 9003; Includes corner wall mount: No; Installation site: ceiling; Installation: In-ceiling installation, Ceiling; IP-rating: IP20; Ambient temperature: -25 – 55 °C; Material: Plastic; Mains power supply: 220 – 240 V / 50 – 60 Hz; Number of Dali users: 20; Steuerausgang, Dali: Broadcast 1x20 electronic ballasts; With bus coupling: No; Technology, sensors: passive infrared, Light sensor; Mounting height: 2 – 5 m; Mounting height max.: 5,00 m; Optimum mounting height: 2,8 m; Detection angle: 360 °; Angle of aperture: 90 °; Sneak-by guard: Yes; Capability of masking out individual segments: Yes; Electronic scalability: No; Mechanical scalability: Yes; Reach, radial: 4 x 4 m (16 m²); Reach, tangential: 6 x 6 m (36 m²); Reach, presence: 4 x 4 m (16 m²); Switching zones: 168 switching zones; Abdeckmaterial Lieferumfang: shrouds; Functions: Semi-/fully automatic, Lighting scenario, Manual ON / ON-OFF, Normal / test mode, Neighbouring group function, TouchDIM function, Motions sensor, Constant-lighting control, Light sensor, Adjustable fade time when switching on and off, Constant-lighting control ON-OFF, Presence function, Presence detector logic; Twilight setting: 2 – 1000 lx; Time setting: 5 sec – 60 min; Basic light level function: Yes; Basic light level function time: 10s-60 min, all night, Brightness-controlled, OFF; Main light adjustable: 0 - 100 %; Twilight setting TEACH: Yes; Constant-lighting control: Yes; Interconnection: Yes; Interconnection via: Bluetooth Mesh Connect; Type DALI output: Single-Master

**Manufacturer** Steinel

**Prod. No.** 067144

**Ordering designation** IR Micro Office 6m DALI-2 APC - in-ceiling installation

Deliver, install and set ready for operation