**STEINEL Professional System components**

**Wireless push button PB2-Bluetooth**

Dimensions (L x W x H): 15 x 81 x 81 mm; With motion detector: No; Manufacturer's Warranty: 5 years; Settings via: Connect Bluetooth Mesh, App; With remote control: No; PU1, EAN: 4007841084653; Type: Other; Application, place: Indoors; Application, room: one-person office, recreation room, function room / ancillary room, open-plan office, hotel room, Indoors, classroom, conference room / meeting room, stairwell; Colour: white; Colour, RAL: 9010; Includes corner wall mount: No; Installation site: wall; Installation: Surface wiring, Other, Wall; IP-rating: IP20; Protection class: without; Ambient temperature: -20 – 40 °C; Switching output 1, floating: No; Switching output 2, floating: No; Power supply, detail: by pressing the rocker switch, current-independent; With bus coupling: No; Sneak-by guard: No; Capability of masking out individual segments: No; Electronic scalability: No; Mechanical scalability: No; Transmitter range: 30 m; Functions: Push button configuration; Basic light level function: No; Main light adjustable: No; Twilight setting TEACH: No; Constant-lighting control: No; Interconnection: Yes; Interconnection via: Bluetooth Mesh Connect

**Manufacturer** Steinel

**Prod. No.** 084653

**Ordering designation** Wireless push button PB2-Bluetooth

Deliver, install and set ready for operation