**STEINEL Professional System components**

**Relais REL5A-DALI-2**

Dimensions (L x W x H): 20 x 46 x 45 mm; With motion detector: No; Manufacturer's Warranty: 5 years; Settings via: App, Bus; With remote control: No; PU1, EAN: 4007841082109; Type: Other; Colour: white; Includes corner wall mount: No; IP-rating: IP20; Ambient temperature: -20 – 50 °C; Mains power supply: 220 – 240 V / 50 – 60 Hz; Switching output 1, resistive: 1000 W; Switching output 1, number of LEDs / fluorescent lamps: 50 pcs.; LED lamps > 8 W: 300 W; Capacitive load in μF: 176 µF; Number of Dali users: 1; With bus coupling: No; Sneak-by guard: No; Capability of masking out individual segments: No; Mechanical scalability: No; Functions: Relay output; Basic light level function: No; Main light adjustable: No; Twilight setting TEACH: No; Constant-lighting control: No; Typical current consumption at 16V input voltage: 2 mA; Max. Current consumption at 10V input voltage in regular operation: 2 mA

**Manufacturer** Steinel

**Prod. No.** 082109

**Ordering designation** Relais REL5A-DALI-2

Deliver, install and set ready for operation