**STEINEL Professional Sensor-switched indoor light**

**RS PRO LED Q1**

**warm white white V2**

Dimensions (L x W x H): 331 x 331 x 56 mm; Mains power supply: 220 – 240 V; Output: 26 W; Luminous flux: 2703 lm; Colour temperature: 3000 K; Colour Rendering Index: 80-89; Lamp: LED cannot be replaced; Base: without; With motion detector: Yes; Photo-cell controller: Yes; Impact resistance: IK00; IP-rating: IP20; Protection class: II; Ambient temperature: -10 – 40 °C; Housing material: Aluminium; Cover material: Plastic, opal; Manufacturer's Warranty: 5 years; Version: warm white white

**Manufacturer** Steinel

**Prod. No.**

**Ordering designation** RS PRO LED Q1 warm white white

Deliver, install and set ready for operation