**STEINEL Professional Motion and Presence Detector**

**IS 3360**

**PF - surface, sq.**

Dimensions (L x W x H): 65 x 95 x 95 mm; With motion detector: Yes; Manufacturer's Warranty: 5 years; Settings via: Remote control, Potentiometers, Smart Remote; With remote control: No; Version: PF - surface, sq.; PU1, EAN: 4007841010515; Type: Motion and Presence Detector; Application, place: Outdoors, Indoors; Application, room: production facilities, recreation room, changing room, function room / ancillary room, sports hall, reception / lobby, stairwell, WC / washroom, multi-storey / underground car park, outdoors, warehouse, Indoors; Colour: white; Colour, RAL: 9003; Includes corner wall mount: No; Installation site: ceiling; Installation: Surface wiring, Ceiling; IP-rating: IP54; Ambient temperature: -20 – 50 °C; Material: Plastic; Mains power supply: 220 – 240 V / 50 – 60 Hz; Fluorescent lamps, electronic ballast: 1500 W; Fluorescent lamps, uncorrected: 1000 VA; Fluorescent lamps, series-corrected: 400 VA; Fluorescent lamps, parallel-corrected: 400 VA; Switching output 1, low-voltage halogen lamps: 2000 VA; LED lamps < 2 W: 100 W; LED lamps > 2 W < 8 W: 300 W; LED lamps > 8 W: 600 W; Capacitive load in μF: 176 µF; Technology, sensors: passive infrared, Light sensor; Mounting height: 2,50 – 4,00 m; Mounting height max.: 4,00 m; Optimum mounting height: 2,8 m; Detection angle: 360 °; Angle of aperture: 180 °; Sneak-by guard: Yes; Capability of masking out individual segments: Yes; Electronic scalability: No; Mechanical scalability: No; Reach, radial: Ø 8 m (50 m²); Reach, tangential: Ø 40 m (1257 m²); Reach, presence: Ø 3 m (7 m²); Switching zones: 1416 switching zones; Functions: Normal / test mode, Manual ON / ON-OFF; Twilight setting: 2 – 1000 lx; Time setting: 5 sec – 15 min; Basic light level function: No; Main light adjustable: No; Twilight setting TEACH: Yes; Constant-lighting control: No; Interconnection: Yes; Type of interconnection: Master/master; Interconnection via: Cable

**Manufacturer** Steinel

**Prod. No.** 010515

**Ordering designation** IS 3360 PF - surface, sq.

Deliver, install and set ready for operation