**STEINEL Professional Motion detector**

**IS 345**

**DALI-2 APC - surface, rd.**

Dimensions (Ø x H): 126 x 65 mm; Manufacturer's Warranty: 5 years; Settings via: Remote control, Potentiometers, Smart Remote; With remote control: No; Version: DALI-2 APC - surface, rd.; PU1, EAN: 4007841033859; Type: Motion detectors; Application, place: Outdoors, Indoors; Application, room: corridor / aisle, multi-storey / underground car park, outdoors, Indoors; Colour: white; Colour, RAL: 9003; Includes corner wall mount: No; Installation site: ceiling; Installation: Surface wiring, Ceiling; IP-rating: IP54; Ambient temperature: -20 – 50 °C; Material: Plastic; Mains power supply: 220 – 240 V / 50 – 60 Hz; Steuerausgang, Dali: Broadcast 1x30 electronic ballasts; Technology, sensors: passive infrared, Light sensor; Mounting height: 2,50 – 5,00 m; Mounting height max.: 5,00 m; Optimum mounting height: 2,8 m; Detection angle: Aisle, 360 °; Angle of aperture: 45 °; Sneak-by guard: Yes; Capability of masking out individual segments: Yes; Electronic scalability: No; Mechanical scalability: No; Reach, radial: 12 x 6 m (72 m²); Reach, tangential: 23 x 6 m (138 m²); Switching zones: 280 switching zones; Functions: Normal / test mode, Manual ON / ON-OFF, Constant-lighting control ON-OFF; Twilight setting: 2 – 1000 lx; Time setting: 5 sec – 15 min; Basic light level function: Yes; Basic light level function time: 1-30 min, all night; Main light adjustable: 50 - 100 %; Twilight setting TEACH: Yes; Constant-lighting control: Yes; Interconnection: Yes; Type of interconnection: Master/slave; Interconnection via: Cable

**Manufacturer** Steinel

**Prod. No.** 033859

**Ordering designation** IS 345 DALI-2 APC - surface, rd.

Deliver, install and set ready for operation